Snow temperature is measured along the cross country and biathlon courses by an infrared sensor mounted on a sled. Position is determined by a GPS unit. Measurements are taken every 5 seconds. For further details, see http:// www.met.utah.edu/olympics or contact jhorel @met.utah.edu.

Obser vations During W inter 2001

M

M

A

A

Snow Temperatur e at Soldier Hollo w Olympic Venue

J. Horel, M. Splitt, D. Myrick NOAA Cooperative Institute for Regional Prediction, University of Utah

Biathlon Course

Cross Country Course

Cross Country Course M

A

A

A

M